0 Technic Beam  9
0 Name: 40490.dat
0 Author: Ross Crawford [rosco]
0 !LDRAW_ORG Part UPDATE 2009-01
0 !LICENSE Redistributable under CCAL version 2.0 : see CAreadme.txt

0 BFC CERTIFY CW

0 !HISTORY 2002-06-11 [PTadmin] Official Update 2002-03
0 !HISTORY 2007-05-04 [PTadmin] Header formatted for Contributor Agreement
0 !HISTORY 2008-07-01 [PTadmin] Official Update 2008-01
0 !HISTORY 2008-07-07 [Philo] Reduced width from 20 to 18 ldu, BFC (2002-07-19)
0 !HISTORY 2008-07-08 [OrionP] Updated to use updated larm primitive (2003-09-11)
0 !HISTORY 2008-07-09 [sbliss] Combined groups of 1-4ring8.dat into single 4-4ring8.dat. Corrected BFC issue of primitives being vertically mirrored (ie, Y components negated); changed those transforms to 180-degree rotations on Z (ie, I negated X components) (2004-10-15)
0 !HISTORY 2008-07-10 [guyvivan] Use more primitives (2004-11-26)
0 !HISTORY 2008-07-11 [PTadmin] Renamed from 120 (2005-07-07)
0 !HISTORY 2009-05-02 [PTadmin] Official Update 2009-01

1 16 0 -10 -80 9 0 0 0 1 0 0 0 -9 2-4edge.dat
1 16 0 10 -80 9 0 0 0 1 0 0 0 -9 2-4edge.dat
1 16 0 -10 -80 9 0 0 0 20 0 0 0 -9 2-4cyli.dat
1 16 0 -10 80 -9 0 0 0 1 0 0 0 9 2-4edge.dat
1 16 0 10 80 -9 0 0 0 1 0 0 0 9 2-4edge.dat
1 16 0 -10 80 -9 0 0 0 20 0 0 0 9 2-4cyli.dat
0 BFC INVERTNEXT
1 16 0 -8 -80 6 0 0 0 16 0 0 0 6 4-4cyli.dat
1 16 0 -10 -80 1 0 0 0 1 0 0 0 1 peghole.dat
1 16 0 10 -80 -1 0 0 0 -1 0 0 0 1 peghole.dat
1 16 0 0 80 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 60 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 40 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 20 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 0 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 -20 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 -40 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 0 -60 1 0 0 0 -1 0 0 0 -1 beamhole.dat
1 16 0 -10 -80 1 0 0 0 1 0 0 0 1 4-4ring8.dat
1 16 0 10 -80 -1 0 0 0 -1 0 0 0 1 4-4ring8.dat
1 16 9 0 0 0 -1 0 0 0 -10 80 0 0 rect2p.dat
1 16 -9 0 0 0 1 0 0 0 -10 -80 0 0 rect2p.dat
0
